; This is a comment.
; config options go here.
forward-zone: name: "." forward-addr: 216.0.0.1
CONFIG_END

SCENARIO_BEGIN Query receives answer from the cache

STEP 1 QUERY
ENTRY_BEGIN
	REPLY RD
	SECTION QUESTION
	www.example.com. IN A
ENTRY_END
; the query is sent to the forwarder - no cache yet.
STEP 2 CHECK_OUT_QUERY
ENTRY_BEGIN
	MATCH qname qtype opcode
	SECTION QUESTION
	www.example.com. IN A
ENTRY_END
STEP 3 REPLY
ENTRY_BEGIN
	MATCH opcode qtype qname
	ADJUST copy_id
	; authoritative answer
	REPLY QR AA RD RA NOERROR
	SECTION QUESTION
	www.example.com. IN A
	SECTION ANSWER
	www.example.com. IN A 10.20.30.40
	SECTION AUTHORITY
	www.example.com. IN NS ns.example.com.
	SECTION ADDITIONAL
	ns.example.com. IN A 10.20.30.50
ENTRY_END
STEP 4 CHECK_ANSWER
ENTRY_BEGIN
	MATCH all 
	REPLY QR RD RA
	SECTION QUESTION
	www.example.com. IN A
	SECTION ANSWER
	www.example.com. IN A 10.20.30.40
	SECTION AUTHORITY
	www.example.com. IN NS ns.example.com.
	SECTION ADDITIONAL
	ns.example.com. IN A 10.20.30.50
ENTRY_END

; another query, same, so it must be answered from the cache
STEP 5 QUERY
ENTRY_BEGIN
	REPLY RD
	SECTION QUESTION
	www.example.com. IN A
ENTRY_END
; immediate answer without an OUT_QUERY happening (checked on exit)
; also, the answer does not have AA set
STEP 6 CHECK_ANSWER
ENTRY_BEGIN
	MATCH all
	REPLY QR RD RA
	SECTION QUESTION
	www.example.com. IN A
	SECTION ANSWER
	www.example.com. IN A 10.20.30.40
	SECTION AUTHORITY
	www.example.com. IN NS ns.example.com.
	SECTION ADDITIONAL
	ns.example.com. IN A 10.20.30.50
ENTRY_END

SCENARIO_END
