; Test subnet option in combination with dnssec
; Client asks for subnet data

server:
	trust-anchor: "example.com.    3600    IN      DS      2854 3 1 46e4ffc6e9a4793b488954bd3f0cc6af0dfb201b"
	val-override-date: "20070916134226"
	trust-anchor-signaling: no
	target-fetch-policy: "0 0 0 0 0"
	send-client-subnet: 1.2.3.4
	max-client-subnet-ipv4: 17
	module-config: "subnetcache validator iterator"
	verbosity: 3
	fake-sha1: yes
	fake-dsa: yes
	qname-minimisation: "no"
	minimal-responses: no

stub-zone:
	name: "."
	stub-addr: 193.0.14.129 	# K.ROOT-SERVERS.NET.
CONFIG_END

SCENARIO_BEGIN Test validator with positive response

; K.ROOT-SERVERS.NET.
RANGE_BEGIN 0 100
	ADDRESS 193.0.14.129 
	ENTRY_BEGIN
		MATCH opcode qtype qname ednsdata
		ADJUST copy_id
		REPLY QR NOERROR
		SECTION QUESTION
			. IN NS
		SECTION ANSWER
			. IN NS	K.ROOT-SERVERS.NET.
		SECTION ADDITIONAL
			HEX_EDNSDATA_BEGIN
				;; we expect to receive empty
			HEX_EDNSDATA_END
			K.ROOT-SERVERS.NET.	IN	A	193.0.14.129
	ENTRY_END

	ENTRY_BEGIN
		MATCH opcode qtype qname
		ADJUST copy_id
		REPLY QR NOERROR
		SECTION QUESTION
			www.example.com. IN A
		SECTION AUTHORITY
			com.	IN NS	a.gtld-servers.net.
		SECTION ADDITIONAL
			a.gtld-servers.net.	IN 	A	192.5.6.30
	ENTRY_END
RANGE_END

; a.gtld-servers.net.
RANGE_BEGIN 0 100
	ADDRESS 192.5.6.30
	ENTRY_BEGIN
		MATCH opcode qtype qname ednsdata
		ADJUST copy_id
		REPLY QR NOERROR
		SECTION QUESTION
			com. IN NS
		SECTION ANSWER
			com.    IN NS   a.gtld-servers.net.
		SECTION ADDITIONAL
			HEX_EDNSDATA_BEGIN
				;; we expect to receive empty
			HEX_EDNSDATA_END
			a.gtld-servers.net.     IN      A       192.5.6.30
	ENTRY_END

	ENTRY_BEGIN
		MATCH opcode qtype qname
		ADJUST copy_id
		REPLY QR NOERROR
		SECTION QUESTION
			www.example.com. IN A
		SECTION AUTHORITY
			example.com.	IN NS	ns.example.com.
		SECTION ADDITIONAL
			ns.example.com.		IN 	A	1.2.3.4
	ENTRY_END
RANGE_END

; ns.example.com.
RANGE_BEGIN 0 100
	ADDRESS 1.2.3.4
	ENTRY_BEGIN
		MATCH opcode qtype qname ednsdata
		ADJUST copy_id
		REPLY QR NOERROR
		SECTION QUESTION
			example.com. IN NS
		SECTION ANSWER
			example.com.    IN NS   ns.example.com.
			example.com.    3600    IN      RRSIG   NS 3 2 3600 20070926134150 20070829134150 2854 example.com. MC0CFQCN+qHdJxoI/2tNKwsb08pra/G7aAIUAWA5sDdJTbrXA1/3OaesGBAO3sI= ;{id = 2854}
		SECTION ADDITIONAL
			HEX_EDNSDATA_BEGIN
				;; we expect to receive empty
			HEX_EDNSDATA_END
			ns.example.com.         IN      A       1.2.3.4
			ns.example.com. 3600    IN      RRSIG   A 3 3 3600 20070926135752 20070829135752 2854 example.com. MC0CFQCMSWxVehgOQLoYclB9PIAbNP229AIUeH0vNNGJhjnZiqgIOKvs1EhzqAo= ;{id = 2854}
	ENTRY_END

	; response to DNSKEY priming query
	ENTRY_BEGIN
		MATCH opcode qtype qname ednsdata
		ADJUST copy_id
		REPLY QR NOERROR
		SECTION QUESTION
			example.com. IN DNSKEY
		SECTION ANSWER
			example.com.    3600    IN      DNSKEY  256 3 3 ALXLUsWqUrY3JYER3T4TBJII s70j+sDS/UT2QRp61SE7S3E EXopNXoFE73JLRmvpi/UrOO/Vz4Se 6wXv/CYCKjGw06U4WRgR YXcpEhJROyNapmdIKSx hOzfLVE1gqA0PweZR8d tY3aNQSRn3sPpwJr6Mi /PqQKAMMrZ9ckJpf1+b QMOOvxgzz2U1GS18b3y ZKcgTMEaJzd/GZYzi/B N2DzQ0MsrSwYXfsNLFO Bbs8PJMW4LYIxeeOe6rUgkWOF 7CC9Dh/dduQ1QrsJhmZAEFfd6ByYV+ ;{id = 2854 (zsk), size = 1688b}
			example.com.    3600    IN      RRSIG   DNSKEY 3 2 3600 20070926134802 20070829134802 2854 example.com. MCwCFG1yhRNtTEa3Eno2zhVVuy2EJX3wAhQeLyUp6+UXcpC5qGNu9tkrTEgPUg== ;{id = 2854}
		SECTION AUTHORITY
			example.com.	IN NS	ns.example.com.
			example.com.    3600    IN      RRSIG   NS 3 2 3600 20070926134150 20070829134150 2854 example.com. MC0CFQCN+qHdJxoI/2tNKwsb08pra/G7aAIUAWA5sDdJTbrXA1/3OaesGBAO3sI= ;{id = 2854}
		SECTION ADDITIONAL
			HEX_EDNSDATA_BEGIN
				;; we expect to receive empty
			HEX_EDNSDATA_END
			ns.example.com.		IN 	A	1.2.3.4
			ns.example.com. 3600    IN      RRSIG   A 3 3 3600 20070926135752 20070829135752 2854 example.com. MC0CFQCMSWxVehgOQLoYclB9PIAbNP229AIUeH0vNNGJhjnZiqgIOKvs1EhzqAo= ;{id = 2854}
	ENTRY_END

	; response to query of interest
	ENTRY_BEGIN
		MATCH opcode qtype qname ednsdata
		ADJUST copy_id
		REPLY QR NOERROR
		SECTION QUESTION
			www.example.com. IN A
		SECTION ANSWER
			www.example.com. IN A	10.20.30.40
			ns.example.com. 3600    IN      RRSIG   A 3 3 3600 20070926134150 20070829134150 2854 example.com. MC0CFQCQMyTjn7WWwpwAR1LlVeLpRgZGuQIUCcJDEkwAuzytTDRlYK7nIMwH1CM= ;{id = 2854}
		SECTION AUTHORITY
			example.com.	IN NS	ns.example.com.
			example.com.    3600    IN      RRSIG   NS 3 2 3600 20070926134150 20070829134150 2854 example.com. MC0CFQCN+qHdJxoI/2tNKwsb08pra/G7aAIUAWA5sDdJTbrXA1/3OaesGBAO3sI= ;{id = 2854}
		SECTION ADDITIONAL
			HEX_EDNSDATA_BEGIN
							; client is 127.0.0.1
				00 08 		; OPC
				00 07 		; option length
				00 01 		; Family
				11 00 		; source mask, scopemask
				7f 00 00 	; address
			HEX_EDNSDATA_END
			ns.example.com.		IN 	A	1.2.3.4
			www.example.com.        3600    IN      RRSIG   A 3 3 3600 20070926134150 20070829134150 2854 example.com. MC0CFC99iE9K5y2WNgI0gFvBWaTi9wm6AhUAoUqOpDtG5Zct+Qr9F3mSdnbc6V4= ;{id = 2854}
	ENTRY_END
RANGE_END

STEP 1 QUERY
ENTRY_BEGIN
	HEX_ANSWER_BEGIN;
		00 00 01 00 00 01 00 00		;ID 0
		00 00 00 01 03 77 77 77		; www.example.com A? (DO)
		07 65 78 61 6d 70 6c 65 
		03 63 6f 6d 00 00 01 00
		01 00 00 29 10 00 00 00 
		80 00 00 0b
		
		00 08 00 07					; OPC, optlen
		00 01 11 00					; ip4, scope 17, source 0
		7f 00 00   					;127.0.0.0/17
	HEX_ANSWER_END
ENTRY_END



; recursion happens here.
STEP 10 CHECK_ANSWER
ENTRY_BEGIN
	MATCH all ednsdata
	REPLY QR RD RA AD NOERROR
	SECTION QUESTION
		www.example.com. IN A
	SECTION ANSWER
		www.example.com. IN A	10.20.30.40
		www.example.com.        3600    IN      RRSIG   A 3 3 3600 20070926134150 20070829134150 2854 example.com. MC0CFC99iE9K5y2WNgI0gFvBWaTi9wm6AhUAoUqOpDtG5Zct+Qr9F3mSdnbc6V4= ;{id = 2854}
	SECTION AUTHORITY
		example.com.	IN NS	ns.example.com.
		example.com.    3600    IN      RRSIG   NS 3 2 3600 20070926134150 20070829134150 2854 example.com. MC0CFQCN+qHdJxoI/2tNKwsb08pra/G7aAIUAWA5sDdJTbrXA1/3OaesGBAO3sI= ;{id = 2854}
	SECTION ADDITIONAL
		HEX_EDNSDATA_BEGIN
						; client is 127.0.0.1
			00 08 		; OPC
			00 07 		; option length
			00 01 		; Family
			11 00 		; source mask, scopemask
			7f 00 00 	; address
		HEX_EDNSDATA_END
		ns.example.com.		IN 	A	1.2.3.4
		ns.example.com. 3600    IN      RRSIG   A 3 3 3600 20070926134150 20070829134150 2854 example.com. MC0CFQCQMyTjn7WWwpwAR1LlVeLpRgZGuQIUCcJDEkwAuzytTDRlYK7nIMwH1CM= ;{id = 2854}
ENTRY_END

SCENARIO_END
